[100]
en=Fan unknow
ch=风扇未知错误

[110]
en=Fan 1 detect speed error
ch=风扇1转速探测错误

[111]
en=Fan 2 detect speed error
ch=风扇2转速检查错误

[120]
en=Fan 1 speed error LV1
ch=风扇1转速检查错误

[121]
en=Fan 2 speed error LV1
ch=风扇2转速检查错误

[130]
en=Fan 1 speed error LV2
ch=风扇1转速检查错误

[131]
en=Fan 2 speed error LV2
ch=风扇2转速检查错误

[140]
en=Fan high percent
ch=风扇转速太高，请检查环境温度

[200]
en=No power found
ch=找不到电源模块

[201]
en=Power detect error
ch=找不到电源模块配置

[202]
en=Power voltage error
ch=电源电压错误

[203]
en=Power protecting
ch=电源保护

[204]
en=Power current protecting
ch=电源电流保护

[205]
en=Power current error
ch=电源电流错误

[206]
en=Power input voltage error
ch=电源电压错误

[207]
en=Power input current protecting
ch=电源输入电流保护

[208]
en=Power power error
ch=电源功率错误

[209]
en=Power voltage offset error
ch=电源电压偏移错误

[210]
en=Power error status
ch=电源状态错误

[211]
en=Power iout error
ch=电源输出电流错误

[212]
en=Power vout error
ch=电源输出电压错误

[213]
en=Power iin or vin or pin error
ch=电源输入电流电压或输入功率错误

[214]
en=Power pin did not change
ch=电源输入功率没有变化

[215]
en=Power vout set error
ch=电源输出设置错误

[217]
en=Power set enable error
ch=电源开关状态错误

[218]
en=Power input voltage is lower than 230V for high power mode
ch=高性能模式电源输入电压低于230V

[233]
en=Power common status error
ch=电源状态错误

[300]
en=Slot 1 temperature sensor not found
ch=算力板1找不到温度传感器

[301]
en=Slot 2 temperature sensor not found
ch=算力板2找不到温度传感器

[302]
en=Slot 3 temperature sensor not found
ch=算力板3找不到温度传感器

[303]
en=Slot 4 temperature sensor not found
ch=算力板4找不到温度传感器

[320]
en=Slot 1 temperature reading error
ch=算力板1读温度传感器错误

[321]
en=Slot 2 temperature reading error
ch=算力板2读温度传感器错误

[322]
en=Slot 3 temperature reading error
ch=算力板3读温度传感器错误

[323]
en=Slot 4 temperature reading error
ch=算力板4读温度传感器错误

[350]
en=Slot 1 temperature protecting!
ch=算力板1温度保护

[351]
en=Slot 2 temperature protecting!
ch=算力板2温度保护

[352]
en=Slot 3 temperature protecting!
ch=算力板3温度保护

[353]
en=Slot 4 temperature protecting!
ch=算力板4温度保护

[380]
en=Humidity sensor not found
ch=找不到湿度传感器

[381]
en=Humidity sensor reading error
ch=读湿度传感器错误

[383]
en=Humidity sensor protecting
ch=湿度传感器保护

[400]
en=EEPROM unknow error
ch=EEPROM 未知错误

[410]
en=Slot 1 detect eeprom error
ch=算力板1 EEPROM 探测错误

[411]
en=Slot 2 detect eeprom error
ch=算力板2 EEPROM 探测错误

[412]
en=Slot 3 detect eeprom error
ch=算力板3 EEPROM 探测错误

[413]
en=Slot 4 detect eeprom error
ch=算力板4 EEPROM 探测错误

[420]
en=Slot 1 parser eeprom error
ch=算力板1 EEPROM 解析错误

[421]
en=Slot 2 parser eeprom error
ch=算力板2 EEPROM 解析错误

[422]
en=Slot 3 parser eeprom error
ch=算力板3 EEPROM 解析错误

[423]
en=Slot 4 parser eeprom error
ch=算力板4 EEPROM 解析错误

[430]
en=Slot 1 chip bin type error
ch=算力板1 芯片类型错误

[431]
en=Slot 2 chip bin type error
ch=算力板2 芯片类型错误

[432]
en=Slot 3 chip bin type error
ch=算力板3 芯片类型错误

[433]
en=Slot 4 chip bin type error
ch=算力板4 芯片类型错误

[440]
en=Slot 1 eeprom chip num error
ch=算力板1 eeprom芯片错误

[441]
en=Slot 2 eeprom chip num error
ch=算力板2 eeprom芯片错误

[442]
en=Slot 3 eeprom chip num error
ch=算力板3 eeprom芯片错误

[443]
en=Slot 4 eeprom chip num error
ch=算力板4 eeprom芯片错误

[450]
en=Slot 1 eeprom xfer error
ch=算力板1 eeprom读写错误

[451]
en=Slot 2 eeprom xfer error
ch=算力板2 eeprom读写错误

[452]
en=Slot 3 eeprom xfer error
ch=算力板3 eeprom读写错误

[453]
en=Slot 4 eeprom xfer error
ch=算力板4 eeprom读写错误

[500]
en=Board unknow error
ch=算力板错误

[510]
en=Slot 1 miner type error
ch=算力板1 与矿机类型不符

[511]
en=Slot 2 miner type error
ch=算力板2 与矿机类型不符

[512]
en=Slot 3 miner type error
ch=算力板3 与矿机类型不符

[513]
en=Slot 4 miner type error
ch=算力板4 与矿机类型不符

[520]
en=Slot 1 chip bin type is different from other
ch=算力板1 芯片类型与其他不符

[521]
en=Slot 2 chip bin type is different from other
ch=算力板2 芯片类型与其他不符

[522]
en=Slot 3 chip bin type is different from other
ch=算力板3 芯片类型与其他不符

[523]
en=Slot 4 chip bin type is different from other
ch=算力板4 芯片类型与其他不符

[530]
en=Slot 1 not found.
ch=找不到算力板1

[531]
en=Slot 2 not found.
ch=找不到算力板2

[532]
en=Slot 3 not found.
ch=找不到算力板3

[533]
en=Slot 4 not found.
ch=找不到算力板4

[540]
en=Slot 1 reading chip id error
ch=算力板1 读chipid错误

[541]
en=Slot 2 reading chip id error
ch=算力板1 读chipid错误

[542]
en=Slot 3 reading chip id error
ch=算力板1 读chipid错误

[543]
en=Slot 4 reading chip id error
ch=算力板1 读chipid错误

[550]
en=Slot 1 have bad chips
ch=算力板1 有坏芯片

[551]
en=Slot 2 have bad chips
ch=算力板2 有坏芯片

[552]
en=Slot 3 have bad chips
ch=算力板3 有坏芯片

[553]
en=Slot 4 have bad chips
ch=算力板4 有坏芯片

[560]
en=Slot 1 loss balance
ch=算力板1 失衡

[561]
en=Slot 2 loss balance
ch=算力板2 失衡

[562]
en=Slot 3 loss balance
ch=算力板3 失衡

[563]
en=Slot 4 loss balance
ch=算力板4 失衡

[570]
en=Slot 1 xfer error chip
ch=算力板1 传输错误

[571]
en=Slot 2 xfer error chip
ch=算力板2 传输错误

[572]
en=Slot 3 xfer error chip
ch=算力板3 传输错误

[573]
en=Slot 4 xfer error chip
ch=算力板4 传输错误

[580]
en=Slot 1 reset error.
ch=算力板1 复位失败

[581]
en=Slot 2 reset error.
ch=算力板2 复位失败

[582]
en=Slot 3 reset error.
ch=算力板3 复位失败

[583]
en=Slot 4 reset error.
ch=算力板4 复位失败

[590]
en=Slot 1 frequency too low.
ch=算力板1 频率太低

[591]
en=Slot 2 frequency too low.
ch=算力板2 频率太低

[592]
en=Slot 3 frequency too low.
ch=算力板3 频率太低

[593]
en=Slot 4 frequency too low.
ch=算力板4 频率太低

[600]
en=Environment temperature is high
ch=环境温度过高

[610]
en=Environment temperature is high for high power mode
ch=高功率模式导致环境温度过高

[700]
en=MAC address invalid
ch=MAC地址错误

[710]
en=Control board rebooted as exception
ch=控制板异常重启

[711]
en=Control board rebooted as exception and cpufreq reduced
ch=控制板异常重启并且cpu频率减少

[712]
en=Control board cpufreq reduced as exception occurred in the past
ch=控制板发生频率异常下降

[800]
en=Btminer checksum error
ch=Btminer文件检验错误

[801]
en=System-monitor checksum error
ch=System-monitor文件检验错误

[802]
en=Remote-daemon checksum error
ch=Remote-daemon文件检验错误

[901]
en=Power rate error
ch=功耗比错误

[2010]
en=All pools disabled, please check the network or pools configure.
ch=所有矿池不能用，请检查网络或矿池配置

[2020]
en=Pool connection failed, user or password error.
ch=矿池连接失败，用户名或密码错误

[2030]
en=Pools rejection rate too high, please check the network or pools config.
ch=矿池拒绝率太高

[2040]
en=Pool warning
ch=矿池警告

[2110]
en=Slot 1 factory test step not pass.
ch=算力板1工厂测试未通过

[2111]
en=Slot 2 factory test step not pass.
ch=算力板2工厂测试未通过

[2112]
en=Slot 3 factory test step not pass.
ch=算力板3工厂测试未通过

[2113]
en=Slot 4 factory test step not pass.
ch=算力板4工厂测试未通过

[2310]
en=Hashrate too low L1
ch=算力太低 L1

[2320]
en=Hashrate too low L2
ch=算力太低 L2

[2340]
en=Hashrate loss L1
ch=算力丢失 L1

[2350]
en=Hashrate loss L2
ch=算力丢失 L2

[5010]
en=Slot 1, chip voltage too low
ch=算力板1芯片电压太低

[5011]
en=Slot 2, chip voltage too low
ch=算力板2芯片电压太低

[5012]
en=Slot 3, chip voltage too low
ch=算力板3芯片电压太低

[5013]
en=Slot 4, chip voltage too low
ch=算力板4芯片电压太低

[5020]
en=Slot 4, chip voltage change
ch=算力板4芯片电压变化

[5021]
en=Slot 4, chip voltage change
ch=算力板4芯片电压变化

[5022]
en=Slot 4, chip voltage change
ch=算力板4芯片电压变化

[5023]
en=Slot 4, chip voltage change
ch=算力板4芯片电压变化

[5030]
en=Slot 1, chip temperature difference is too large
ch=算力板1芯片温度差距过大

[5031]
en=Slot 2, chip temperature difference is too large
ch=算力板2芯片温度差距过大

[5032]
en=Slot 3, chip temperature difference is too large
ch=算力板3芯片温度差距过大

[5033]
en=Slot 4, chip temperature difference is too large
ch=算力板4芯片温度差距过大

[5040]
en=Slot 1, chip hottest temperature difference is too large
ch=算力板1芯片最高温度差距过大

[5041]
en=Slot 2, chip hottest temperature difference is too large
ch=算力板2芯片最高温度差距过大

[5042]
en=Slot 3, chip hottest temperature difference is too large
ch=算力板3芯片最高温度差距过大

[5043]
en=Slot 4, chip hottest temperature difference is too large
ch=算力板4芯片最高温度差距过大

[5110]
en=Slot 1, upfreq timeout
ch=算力板1升频超时

[5111]
en=Slot 2, upfreq timeout
ch=算力板2升频超时

[5112]
en=Slot 3, upfreq timeout
ch=算力板3升频超时

[5113]
en=Slot 4, upfreq timeout
ch=算力板4升频超时

[520000]
en=Slot 1, chip error nonce
ch=算力板1 芯片nonce错误

[520001]
en=Slot 2, chip error nonce
ch=算力板2 芯片nonce错误

[520002]
en=Slot 3, chip error nonce
ch=算力板3 芯片nonce错误

[520003]
en=Slot 4, chip error nonce
ch=算力板4 芯片nonce错误

[530000]
en=Slot 1, chip few nonce
ch=算力板1 芯片nonce太少

[530001]
en=Slot 2, chip few nonce
ch=算力板2 芯片nonce太少

[530002]
en=Slot 3, chip few nonce
ch=算力板3 芯片nonce太少

[530003]
en=Slot 4, chip few nonce
ch=算力板4 芯片nonce太少

[540000]
en=Slot 1, chip temp protected
ch=算力板1 芯片温度保护

[540001]
en=Slot 2, chip temp protected
ch=算力板2 芯片温度保护

[540002]
en=Slot 3, chip temp protected
ch=算力板3 芯片温度保护

[540003]
en=Slot 4, chip temp protected
ch=算力板4 芯片温度保护

[8410]
en=Firmware chip error
ch=固件对应芯片错误

[9999]
en=Unknow error
ch=未知错误

[8000]
en=The tool version is too low,please download the latest!
ch=工具版本过低，请下载最新工具！


[100000]
en=Security library error
ch=安全模块库错误

[100001]
en=Security error
ch=安全模块错误

[100002]
en=Security error
ch=安全模块错误

[100003]
en=Security error
ch=安全模块错误

[100100]
en=Security btminer be removed
ch=Btminer被删除

[110000]
en=Security illegal file
ch=非法文件

[110001]
en=Security virus 0001 is removed
ch=病毒识别并且被删除
