[100]
en=Fan unknow
ch=风扇未知错误

[110]
en=Intake Fan detect speed error
ch=进风口风扇转速探测错误

[111]
en=Outtake Fan detect speed error
ch=出风口风扇转速探测错误

[120]
en=Intake Fan speed error
ch=进风口风扇转速检查错误

[121]
en=Outtake Fan speed error
ch=出风口风扇转速检查错误

[130]
en=Intake Fan speed error
ch=进风口风扇转速检查错误

[131]
en=Outtake Fan speed error
ch=出风口风扇转速检查错误

[140]
en=Fan high percent, please improve the environment temperature
ch=风扇转速太高，请降低环境温度

[200]
en=No power found, upgrade firmware or replace the PSU
ch=电源检测异常，请升级固件或更换电源

[201]
en=Power detect error, upgrade firmware
ch=找不到电源模块配置，请升级固件

[202]
en=Power voltage error, upgrade firmware
ch=电源电压错误，请升级固件

[203]
en=Power protecting, improve PSU temperature
ch=电源保护，请加强电源散热

[204]
en=Power current protecting, improve PSU temperature
ch=电源电流保护，请加强电源散热

[205]
en=Power current error, check whether the input voltage is stable
ch=电源电流异常，请检查供电电压是否稳定

[206]
en=Power input voltage error, improve your input voltage
ch=电源电压错误，请改善输入电压

[207]
en=Power input current protecting, improve your input voltage
ch=电源输入电流保护，请提高输入电压

[208]
en=Power power error
ch=电源功率错误

[209]
en=Power voltage offset error
ch=电源电压偏移错误

[210]
en=Power error status, please check the Errors on web page
ch=电源状态错误，请查看网页后台错误码

[211]
en=Power iout error, please reboot and check
ch=电源输出电流错误，请尝试重启

[212]
en=Power vout error, please reboot and check
ch=电源输出电压错误，请尝试重启

[213]
en=Power iin or vin or pin error, please reboot or replace the PSU
ch=电源输入电流电压或输入功率错误，请尝试重启或更换电源

[214]
en=Power pin did not change
ch=电源输入功率没有变化

[215]
en=Power vout set error
ch=电源输出设置错误

[216]
en=Power remained unchanged for a long time
ch=电源功率长时间没变化

[217]
en=Power set enable error, please reboot and check
ch=电源开关状态错误，请尝试重启

[218]
en=Power input voltage is lower than 230V for High power mode
ch=高性能模式电源输入电压低于230V

[233]
en=Power over heat error, please improve the PSU temperature
ch=电源过温保护，请改善电源温度

[236]
en=Power over current error, please check whether the screws of power bridge are locked in place
ch=电源过流保护，请检查铜排螺丝是否打紧

[246]
en=Power over current error, please replace the PSU
ch=电源严重过流，请更换电源

[250]
en=Power input voltage is too low, please improve the input voltage
ch=电源欠压保护，请改善输入电压

[251]
en=Power input voltage is too low, please improve the input voltage
ch=电源欠压保护，请改善输入电压

[253]
en=PSU fan detection error
ch=电源风扇异常

[254]
en=PSU fan detection error
ch=电源风扇异常

[257]
en=Power over current protection, please reboot or replace the PSU
ch=电源原边输入过流保护，请尝试重启或更换电源

[263]
en=Power communication error, please check whether the screws of control board are locked in place 
ch=电源通讯错误，请检查控制板固定螺丝是否锁好

[264]
en=Power communication error, please check whether the screws of control board are locked in place 
ch=电源通讯错误，请检查控制板固定螺丝是否锁好

[270]
en=Power input voltage is too high, please check the input voltage
ch=电源过压保护，请检查输入电压

[274]
en=PSU fan warning, please check whether PSU fan is blocked
ch=电源风扇警告，请检查电源风扇是否受阻

[275]
en=Power over heat error, please improve the PSU temperature
ch=电源过温保护，请改善电源温度

[300]
en=Slot 0 temperature sensor not found, please check the adaptor bridge and connection ribbons
ch=0号算力板找不到温度传感器，检查转接板及排线

[301]
en=Slot 1 temperature sensor not found, please check the adaptor bridge and connection ribbons
ch=1号算力板找不到温度传感器，检查转接板及排线

[302]
en=Slot 2 temperature sensor not found, please check the adaptor bridge and connection ribbons
ch=2号算力板找不到温度传感器，检查转接板及排线

[303]
en=Slot 3 temperature sensor not found, please check the adaptor bridge and connection ribbons
ch=3号算力板找不到温度传感器，检查转接板及排线

[320]
en=Slot 0 temperature reading error, please check whether the screws of control board are locked in place 
ch=0号算力板通讯错误，请检查控制板固定螺丝是否锁好

[321]
en=Slot 1 temperature reading error, please check whether the screws of control board are locked in place 
ch=1号算力板通讯错误，请检查控制板固定螺丝是否锁好

[322]
en=Slot 2 temperature reading error, please check whether the screws of control board are locked in place 
ch=2号算力板通讯错误，请检查控制板固定螺丝是否锁好

[323]
en=Slot 3 temperature reading error, please check whether the screws of control board are locked in place 
ch=3号算力板通讯错误，请检查控制板固定螺丝是否锁好

[350]
en=Slot 0 temperature protecting, please improve the hash board temperature
ch=0号算力板温度保护，请降低算力板温度

[351]
en=Slot 1 temperature protecting, please improve the hash board temperature
ch=1号算力板温度保护，请降低算力板温度

[352]
en=Slot 2 temperature protecting, please improve the hash board temperature
ch=2号算力板温度保护，请降低算力板温度

[353]
en=Slot 3 temperature protecting, please improve the hash board temperature
ch=3号算力板温度保护，请降低算力板温度

[380]
en=Humidity sensor not found
ch=找不到湿度传感器

[381]
en=Humidity sensor reading error
ch=读湿度传感器错误

[382]
en=Humidity sensor reading error
ch=读湿度传感器错误

[383]
en=Humidity sensor protecting
ch=湿度传感器保护

[400]
en=EEPROM unknow error
ch=EEPROM 未知错误

[410]
en=Slot 0 detect eeprom error, please check the adaptor bridge and connection ribbons
ch=0号算力板EEPROM探测错误，检查转接板及排线

[411]
en=Slot 1 detect eeprom error, please check the adaptor bridge and connection ribbons
ch=1号算力板EEPROM探测错误，检查转接板及排线

[412]
en=Slot 2 detect eeprom error, please check the adaptor bridge and connection ribbons
ch=2号算力板EEPROM探测错误，检查转接板及排线

[413]
en=Slot 3 detect eeprom error, please check the adaptor bridge and connection ribbons
ch=3号算力板EEPROM探测错误，检查转接板及排线

[420]
en=Slot 0 parser eeprom error, upgrade firmware
ch=0号算力板EEPROM解析错误，请升级固件

[421]
en=Slot 1 parser eeprom error, upgrade firmware
ch=1号算力板EEPROM解析错误，请升级固件

[422]
en=Slot 2 parser eeprom error, upgrade firmware
ch=2号算力板EEPROM解析错误，请升级固件

[423]
en=Slot 3 parser eeprom error, upgrade firmware
ch=3号算力板EEPROM解析错误，请升级固件

[430]
en=Slot 0 chip bin type error
ch=算力板0 芯片类型错误

[431]
en=Slot 1 chip bin type error
ch=算力板1 芯片类型错误

[432]
en=Slot 2 chip bin type error
ch=算力板2 芯片类型错误

[433]
en=Slot 3 chip bin type error
ch=算力板3 芯片类型错误

[440]
en=Slot 0 eeprom chip num error
ch=算力板0 eeprom芯片错误

[441]
en=Slot 1 eeprom chip num error
ch=算力板1 eeprom芯片错误

[442]
en=Slot 2 eeprom chip num error
ch=算力板2 eeprom芯片错误

[443]
en=Slot 3 eeprom chip num error
ch=算力板3 eeprom芯片错误

[450]
en=Slot 0 eeprom xfer error
ch=算力板0 eeprom读写错误

[451]
en=Slot 1 eeprom xfer error
ch=算力板1 eeprom读写错误

[452]
en=Slot 2 eeprom xfer error
ch=算力板2 eeprom读写错误

[453]
en=Slot 3 eeprom xfer error
ch=算力板3 eeprom读写错误

[500]
en=Board unknow error
ch=算力板错误

[510]
en=Slot 0 miner type error
ch=算力板0 与机器类型不符

[511]
en=Slot 1 miner type error
ch=算力板1 与机器类型不符

[512]
en=Slot 2 miner type error
ch=算力板2 与机器类型不符

[513]
en=Slot 3 miner type error
ch=算力板3 与机器类型不符

[520]
en=Slot 0 chip bin type is different from other
ch=算力板0 芯片类型与其他不符

[521]
en=Slot 1 chip bin type is different from other
ch=算力板1 芯片类型与其他不符

[522]
en=Slot 2 chip bin type is different from other
ch=算力板2 芯片类型与其他不符

[523]
en=Slot 3 chip bin type is different from other
ch=算力板3 芯片类型与其他不符

[530]
en=Slot 0 not found.
ch=找不到算力板0

[531]
en=Slot 1 not found.
ch=找不到算力板1

[532]
en=Slot 2 not found.
ch=找不到算力板2

[533]
en=Slot 3 not found.
ch=找不到算力板3

[540]
en=Slot 0 reading chip id error, please replace the adaptor bridge or ribbon
ch=算力板0 读chipid错误，请尝试更换转接板或排线

[541]
en=Slot 1 reading chip id error, please replace the adaptor bridge or ribbon
ch=算力板1 读chipid错误，请尝试更换转接板或排线

[542]
en=Slot 2 reading chip id error, please replace the adaptor bridge or ribbon
ch=算力板2 读chipid错误，请尝试更换转接板或排线

[543]
en=Slot 3 reading chip id error, please replace the adaptor bridge or ribbon
ch=算力板3 读chipid错误，请尝试更换转接板或排线

[550]
en=Slot 0 have bad chips
ch=算力板0 有坏芯片

[551]
en=Slot 1 have bad chips
ch=算力板1 有坏芯片

[552]
en=Slot 2 have bad chips
ch=算力板2 有坏芯片

[553]
en=Slot 3 have bad chips
ch=算力板4 有坏芯片

[560]
en=Slot 0 loss balance, please replace the adaptor bridge or ribbon
ch=算力板0 失衡，请尝试更换转接板或排线

[561]
en=Slot 1 loss balance, please replace the adaptor bridge or ribbon
ch=算力板1 失衡，请尝试更换转接板或排线

[562]
en=Slot 2 loss balance, please replace the adaptor bridge or ribbon
ch=算力板2 失衡，请尝试更换转接板或排线

[563]
en=Slot 3 loss balance, please replace the adaptor bridge or ribbon
ch=算力板3 失衡，请尝试更换转接板或排线

[570]
en=Slot 0 xfer error chip
ch=算力板0 传输错误

[571]
en=Slot 1 xfer error chip
ch=算力板1 传输错误

[572]
en=Slot 2 xfer error chip
ch=算力板2 传输错误

[573]
en=Slot 3 xfer error chip
ch=算力板3 传输错误

[580]
en=Slot 0 reset error.
ch=算力板0 复位失败

[581]
en=Slot 1 reset error.
ch=算力板1 复位失败

[582]
en=Slot 2 reset error.
ch=算力板2 复位失败

[583]
en=Slot 3 reset error.
ch=算力板3 复位失败

[590]
en=Slot 0 frequency too low.
ch=算力板0 频率太低

[591]
en=Slot 1 frequency too low.
ch=算力板1 频率太低

[592]
en=Slot 2 frequency too low.
ch=算力板2 频率太低

[593]
en=Slot 3 frequency too low.
ch=算力板3 频率太低

[600]
en=Environment temperature is high, please improve the environment temperature
ch=环境温度过高，请降低环境温度，加强通风

[610]
en=Environment temperature is high for high power mode
ch=高功率模式导致环境温度过高

[700]
en=MAC address invalid
ch=MAC地址错误

[710]
en=Control board rebooted as exception, please upgrade the firmware
ch=控制板异常重启，请升级固件

[711]
en=Control board rebooted as exception and cpufreq reduced, please upgrade the firmware
ch=控制板异常重启，请升级固件

[712]
en=Control board cpufreq reduced as exception occurred in the past, please upgrade the firmware
ch=控制板发生频率异常下降，请升级固件

[800]
en=Btminer checksum error, please re-upgrade the firmware
ch=Btminer文件检验错误，请重新升级固件

[801]
en=System-monitor checksum error, please re-upgrade the firmware
ch=System-monitor文件检验错误，请重新升级固件

[802]
en=Remote-daemon checksum error, please re-upgrade the firmware
ch=Remote-daemon文件检验错误，请重新升级固件

[901]
en=Power rate error
ch=功耗比错误

[2010]
en=All pools disabled, please check the network or change the pools configure.
ch=所有pool不能用，请检查网络或更换pool配置

[2020]
en=Pool 1 connection failed, user or password error.
ch=pool1连接失败，用户名或密码错误

[2021]
en=Pool 2 connection failed, user or password error.
ch=pool2连接失败，用户名或密码错误

[2022]
en=Pool 3 connection failed, user or password error.
ch=pool3连接失败，用户名或密码错误

[2030]
en=Pools rejection rate too high, please check the network or pools config.
ch=pool拒绝率太高，请检查网络或咨询客服

[2040]
en=Pool lacks important feature
ch=pool缺少重要特性

[2110]
en=Slot 0 factory test step not pass.
ch=算力板0工厂测试未通过

[2111]
en=Slot 1 factory test step not pass.
ch=算力板1工厂测试未通过

[2112]
en=Slot 2 factory test step not pass.
ch=算力板2工厂测试未通过

[2113]
en=Slot 3 factory test step not pass.
ch=算力板3工厂测试未通过

[2310]
en=Hashrate too low, please reboot and check again
ch=算力太低，请尝试重启

[2320]
en=Hashrate too low, please reboot and check again
ch=算力太低，请尝试重启

[2340]
en=Hashrate loss, please reboot and check again
ch=算力丢失，请尝试重启

[2350]
en=Hashrate loss, please reboot and check again
ch=算力丢失，请尝试重启

[5010]
en=Slot 0, chip voltage too low
ch=算力板0芯片电压太低

[5011]
en=Slot 1, chip voltage too low
ch=算力板1芯片电压太低

[5012]
en=Slot 2, chip voltage too low
ch=算力板2芯片电压太低

[5013]
en=Slot 3, chip voltage too low
ch=算力板3芯片电压太低

[5020]
en=Slot 0, chip voltage change
ch=算力板0芯片电压变化

[5021]
en=Slot 1, chip voltage change
ch=算力板1芯片电压变化

[5022]
en=Slot 2, chip voltage change
ch=算力板2芯片电压变化

[5023]
en=Slot 3, chip voltage change
ch=算力板3芯片电压变化

[5030]
en=Slot 0, chip temperature difference is too large
ch=算力板0芯片温度差距过大

[5031]
en=Slot 1, chip temperature difference is too large
ch=算力板1芯片温度差距过大

[5032]
en=Slot 2, chip temperature difference is too large
ch=算力板2芯片温度差距过大

[5033]
en=Slot 3, chip temperature difference is too large
ch=算力板3芯片温度差距过大

[5040]
en=Slot 0, chip hottest temperature difference is too large
ch=算力板0芯片最高温度差距过大

[5041]
en=Slot 1, chip hottest temperature difference is too large
ch=算力板1芯片最高温度差距过大

[5042]
en=Slot 2, chip hottest temperature difference is too large
ch=算力板2芯片最高温度差距过大

[5043]
en=Slot 3, chip hottest temperature difference is too large
ch=算力板3芯片最高温度差距过大

[5110]
en=Slot 0, upfreq timeout
ch=算力板0升频超时

[5111]
en=Slot 1, upfreq timeout
ch=算力板1升频超时

[5112]
en=Slot 2, upfreq timeout
ch=算力板2升频超时

[5113]
en=Slot 3, upfreq timeout
ch=算力板3升频超时

[520001]
en=Slot 0 chip 1 error nonce
ch=算力板0 芯片1 nonce错误

[520002]
en=Slot 0, chip 2 error nonce
ch=算力板0 芯片2 nonce错误

[520003]
en=Slot 0, chip 3 error nonce
ch=算力板0 芯片3 nonce错误


[521001]
en=Slot 1 chip 1 error nonce
ch=算力板1 芯片1 nonce错误

[521002]
en=Slot 1, chip 2 error nonce
ch=算力板1 芯片2 nonce错误

[521003]
en=Slot 1, chip 3 error nonce
ch=算力板1 芯片3 nonce错误


[522001]
en=Slot 2 chip 1 error nonce
ch=算力板2 芯片1 nonce错误

[522002]
en=Slot 2, chip 2 error nonce
ch=算力板2 芯片2 nonce错误

[522003]
en=Slot 2, chip 3 error nonce
ch=算力板2 芯片3 nonce错误



[523000]
en=Slot 3, chip error nonce
ch=算力板3 芯片nonce错误

[523001]
en=Slot 3 chip 1 error nonce
ch=算力板3 芯片1 nonce错误

[523002]
en=Slot 3, chip 2 error nonce
ch=算力板3 芯片2 nonce错误

[523003]
en=Slot 3, chip 3 error nonce
ch=算力板3 芯片3 nonce错误


[530001]
en=Slot 0, chip 1 few nonce
ch=算力板0 芯片1nonce太少

[530002]
en=Slot 0, chip 2 few nonce
ch=算力板0 芯片2nonce太少

[530003]
en=Slot 0, chip 3 few nonce
ch=算力板0 芯片3nonce太少


[531001]
en=Slot 1, chip 1 few nonce
ch=算力板1 芯片1nonce太少

[531002]
en=Slot 1, chip 2 few nonce
ch=算力板1 芯片2nonce太少

[531003]
en=Slot 1, chip 3 few nonce
ch=算力板1 芯片3nonce太少

[532001]
en=Slot 2, chip 1 few nonce
ch=算力板2 芯片1nonce太少

[532002]
en=Slot 2, chip 2 few nonce
ch=算力板2 芯片2nonce太少

[532003]
en=Slot 2, chip 3 few nonce
ch=算力板2 芯片3nonce太少


[533001]
en=Slot 3, chip 1 few nonce
ch=算力板3 芯片1nonce太少

[533002]
en=Slot 3, chip 2 few nonce
ch=算力板3 芯片2nonce太少

[533003]
en=Slot 3, chip 3 few nonce
ch=算力板3 芯片3nonce太少


[540000]
en=Slot 0, chip temp protected
ch=算力板0 芯片温度保护

[540001]
en=Slot 1, chip temp protected
ch=算力板1 芯片温度保护

[540002]
en=Slot 2, chip temp protected
ch=算力板2 芯片温度保护

[540003]
en=Slot 3, chip temp protected
ch=算力板3 芯片温度保护



[540000]
en=Slot 0, chip temp protected
ch=算力板0 芯片温度保护

[540001]
en=Slot 0, chip 1 temp protected
ch=算力板0 芯片温度保护

[540002]
en=Slot 0, chip 2 temp protected
ch=算力板0 芯片温度保护

[540003]
en=Slot 0, chip 3 temp protected
ch=算力板3 芯片3温度保护




[541000]
en=Slot 1, chip temp protected
ch=算力板1 芯片温度保护

[541001]
en=Slot 1, chip 1 temp protected
ch=算力板1 芯片温度保护

[541002]
en=Slot 1, chip 2 temp protected
ch=算力板1 芯片温度保护

[541003]
en=Slot 1, chip 3 temp protected
ch=算力板1 芯片3温度保护



[542000]
en=Slot 2, chip temp protected
ch=算力板2 芯片温度保护

[542001]
en=Slot 2, chip 1 temp protected
ch=算力板2 芯片温度保护

[542002]
en=Slot 2, chip 2 temp protected
ch=算力板2 芯片温度保护

[542003]
en=Slot 2, chip 3 temp protected
ch=算力板2 芯片3温度保护



[543000]
en=Slot 3, chip temp protected
ch=算力板3 芯片温度保护

[543001]
en=Slot 3, chip 1 temp protected
ch=算力板3 芯片温度保护

[543002]
en=Slot 3, chip 2 temp protected
ch=算力板3 芯片温度保护

[543003]
en=Slot 3, chip 3 temp protected
ch=算力板3 芯片3温度保护


[8410]
en=Firmware chip error, please upgrade firmware
ch=固件对应芯片错误，请升级固件

[9999]
en=Unknow error
ch=未知错误

[8000]
en=The tool version is too low, please download the latest!
ch=工具版本过低，请下载最新工具！


[100000]
en=Security library error, please upgrade firmware
ch=安全模块库错误，请升级固件

[100001]
en=Security error, please upgrade firmware
ch=安全模块错误，请升级固件

[100002]
en=Security error, please upgrade firmware
ch=安全模块错误，请升级固件

[100003]
en=Security error, please upgrade firmware
ch=安全模块错误，请升级固件

[100100]
en=Security btminer be removed, please upgrade firmware
ch=Btminer被删除，请升级固件

[110000]
en=Security illegal file, please upgrade firmware
ch=非法文件，请升级固件

[110001]
en=Security virus 0001 is removed, please upgrade firmware
ch=病毒识别并且被删除，请升级固件
