

SetIP User manual

1. Put the tool on the PC which is connect with the same router with the miner, then double click the tool and choose the language.



1. Report the miner IP



Press the IPset button 1 to 2 seconds then the IP of the miner will show here

1. Set all the miner to Static IP and make the IP relate to the location as the follow picture.

